RV国际版详情页
产品名称：
RV Plus Series Insulation Shipper
产品简介：
The RV Plus Series, developed by CCTS CHINA, stands as a paragon of innovation in the realm of shipping insulation. This series of shippers is not only reusable but also highly cost - effective, powered by advanced PCM (Phase - Change Material) ice packs. Its design features straightforward and proven modularity, guaranteeing excellent thermal performance that can last anywhere from 7 to 10 days. What's more, it functions optimally throughout the year, even in the most extreme temperature conditions.
Switch Temperature Freely by PCM：
【E】-30℃～-20℃      【K】-25℃～-15℃         【B】-20℃～-10℃
【J】-10℃～0℃          【F】0℃～+4℃/+5℃      【C】+2℃～+8℃
【D】+15℃～+25℃    【N】+25℃～+35℃        【U】+50℃～+60℃
Feature：
· 10 days cooling presevation performance 
· Pre-qualified according to ISTA, WHO,GSP
· Easy to Use and Assemble with detailed 3D manual and SOP maunal
· Shock aborbent, Damage resistant,Economical
· Custom sizing, insulation material and thicknesses, and printing available
	产品型号
	控温范围
	保温时长
	有效容积（L）

	NB4D-RV31A
	2℃~8℃、15℃~25℃、-25℃~-15℃
	96h
	31.7 

	NB4D-RV66A
	2℃~8℃、15℃~25℃、-25℃~-15℃
	96h
	67.2 

	NC7D-RV35H
	2℃~8℃、15℃~25℃、-25℃~-15℃
	168h
	28.8 

	NC10D-RV65H
	2℃~8℃、15℃~25℃、-25℃~-15℃
	240h
	60.3 

	NC10D-RV110H
	2℃~8℃、15℃~25℃、-25℃~-15℃
	240h
	103.2 



Application:
Suitable for international transportation of vaccines, drugs, reagents, sensitive chemicals, and electronic components.
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